## Таблица сравнения характеристик коммутаторов SNR и аналогов Cisco

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Модель коммутатора** | **L2** | **L3** | **Кол-во портов 10/100/1000BaseT с поддержкой PoE 802.3at/af** | **Порты****SFP** | **Порты****SFP+** | **Суммарная мощность POE** | **Порты Combo****10/100/1000BaseT****100/1000BaseX SFP** | **Производительность коммутации** | **Возможность****стекирования** | **Поддержка промышленных стандартов** |
| [SNR-S2995G-48TX-POE](https://plcontroller.ru/product/upravlyaemij-poe-kommutator-3urovnya-snr-s2995g-48tx-poe/) | + | + | 48 | 4 | 4 | 740W | - | 176Gbps | + | - |
| [Cisco C9200L-48P-4X](https://www.cisco.com/c/en/us/products/collateral/switches/catalyst-9200-series-switches/nb-06-cat9200-ser-data-sheet-cte-en.html) | + | + | 48 | 4 | 4 | 740W | - | 176Gbps | + | - |
| [SNR-S2995G-24TX-POE](https://plcontroller.ru/product/upravlyaemij-poe-kommutator-3urovnya-snr-s2995g-24tx-poe/) | + | + | 24 | 4 | 4 | 370W | 4 | 128Gbps | + | - |
| [Cisco C9200L-24P-4X](https://www.cisco.com/c/en/us/products/collateral/switches/catalyst-9200-series-switches/nb-06-cat9200-ser-data-sheet-cte-en.html) | + | + | 24 | 4 | 4 | 370W | - | 128Gbps | + | - |
| [SNR-S2985G-24T-POE-E](https://plcontroller.ru/product/upravlyaemij-poe-kommutator-2urovnya-snr-s2985g-24t-poe-e/) | + | - | 24 | 4 | - | 370W | - | 56Gbps | - | - |
| [Cisco C1000-24FP-4G-L](https://www.cisco.com/c/en/us/products/collateral/switches/catalyst-1000-series-switches/nb-06-cat1k-ser-switch-ds-cte-en.html) | + | - | 24 | 4 | - | 370W | - | 56Gbps | - | - |
| [SNR-S2982G-24T-POE](https://plcontroller.ru/product/upravlyaemij-poe-kommutator-2urovnya-snr-s2982g-24t-poe-%D0%BA/) | + | - | 24 | 4 | - | 185W | - | 56Gbps | - | - |
| [Cisco C1000-24P-4G-L](https://www.cisco.com/c/en/us/products/collateral/switches/catalyst-1000-series-switches/nb-06-cat1k-ser-switch-ds-cte-en.html) | + | - | 24 | 4 | - | 195W | - | 56Gbps | - | - |
| [SNR-S2985G-8T-POE](https://plcontroller.ru/product/upravlyaemij-poe-kommutator-2snr-s2985g-8t/) | + | - | 8 | 2 | - | 124W | - | 20Gbps | - | - |
| [Cisco C1000-8FP-E-2G-L](https://www.cisco.com/c/en/us/products/collateral/switches/catalyst-1000-series-switches/nb-06-cat1k-ser-switch-ds-cte-en.html) | + | - | 8 | 2 | - | 120W | 2 | 20Gbps | - | - |
| [SNR-S225Gi-8T-POE](https://plcontroller.ru/product/upravlyaemij-promischlennij-poe-kommutator-snr-s225gi-8t-poe/) | + | - | 8 | 2 | - | 180W | - | 20Gbps | - | + |
| [Cisco IE-3200-8P2S-E](https://www.cisco.com/c/en/us/support/switches/catalyst-ie-3200-8p2s-e-rugged-switch/model.html) | + | - | 8 | 2 | - | 240W | - | 20Gbps | - | + |